,Model##Other##,Nominal Capacity##other##,Sensible Cooling Capacity##HVAC_COOLING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,Electrical_Wattage##ELECTRICAL_WATTAGE##WATTS,EER##other##,IEER##other##,Dead Weight##other##
15 Ton,50GEQ17,15 Ton,178000,15600,17.3,0,1925
