,Model##Other##,Description##Other##,Refrigerant Used##other##,Nominal Capacity##other##,Sensible Cooling Capacity##HVAC_COOLING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,Height##length##inches,Electrical_Wattage##ELECTRICAL_WATTAGE##WATTS,SEER##other##,EER##other##,IEER##other##,Standards Conformance##other##,Efficiency Ratings##other##,Dead Weight##other##
7 Ton,48GCxx07xxx,Carrier Packaged Rooftop Unit - Weathermaker Gas Heat 48GC as Specified,Puron R-410A,6 Ton,72000,1048mm,5900,0,12.2,17.5,ASHRAE 90.1  ;  AHRI 340/360  ;  DOE 2023,82,775
8 Ton,48GCxx08xxx,Carrier Packaged Rooftop Unit - Weathermaker Gas Heat 48GC as Specified,Puron R-410A,7.5 Ton,90000,1253mm,7500,0,12,17.5,ASHRAE 90.1  ;  AHRI 340/360  ;  DOE 2023,82,893
9 Ton,48GCxx09xxx,Carrier Packaged Rooftop Unit - Weathermaker Gas Heat 48GC as Specified,Puron R-410A,8.5 Ton,96000,1253mm,8100,0,11.8,17.3,ASHRAE 90.1  ;  AHRI 340/360  ;  DOE 2023,82,893
