,Model##Other##,Description##Other##,Refrigerant Used##other##,Nominal Capacity##other##,Sensible Cooling Capacity##HVAC_COOLING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,Height##length##inches,Electrical_Wattage##ELECTRICAL_WATTAGE##WATTS,SEER##other##,EER##other##,IEER##other##,Standards Conformance##other##,Efficiency Ratings##other##,Dead Weight##other##
12 Ton,48GCxx12xxx,Carrier Packaged Rooftop Unit - Weathermaker Gas Heat 48GC as Specified,Puron R-410A,10 Ton,114000,1253mm,10000,0,11.4,17.2,ASHRAE 90.1  ;  AHRI 340/360  ;  DOE 2023,82,1037
