# This is a Revit shared parameter file.
# Do not edit manually.
*META	VERSION	MINVERSION
META	2	1
*GROUP	ID	NAME
GROUP	1	Dimensions
GROUP	5	Electrical
GROUP	6	Mechanical
GROUP	8	Identity Data
GROUP	10	Electrical - Loads
GROUP	11	Mechanical - Air Flow
GROUP	12	Energy Analysis
GROUP	14	Mechanical - Loads
GROUP	15	Structural
GROUP	16	Plumbing
GROUP	17	Green Building Properties
GROUP	18	Materials and Finishes
GROUP	19	Other
GROUP	20	Construction
GROUP	22	Constraints
*PARAM	GUID	NAME	DATATYPE	DATACATEGORY	GROUP	VISIBLE
PARAM	4a631e00-98ce-4a8b-85c6-b77e33183f1e	Fan Quantity	INTEGER		6	1
PARAM	aad7c100-5cd6-46de-a224-3bb04707986a	Refrigerant Suction Gas Connection Diameter	PIPE_SIZE		1	1
PARAM	3322e901-ca02-42fe-a7f2-db576614a4d7	Compressor Quantity	INTEGER		6	1
PARAM	ced7b602-d099-4061-8fc5-10774f7d8808	Exhaust Fan	YESNO		6	1
PARAM	09cad502-74ab-4945-9a53-5522ab109284	Actual Refrigerant 2 Flow	PIPING_FLOW		6	1
PARAM	004b0c03-b772-4d7d-8726-cf5c55d2c150	Clearance Offset Front	LENGTH		22	1
PARAM	e56f2f04-58ff-4786-9d0e-977ceeea6ac5	Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	6d3c6004-dce9-4ccf-9320-148946c8b5bc	Heating Seasonal Performance Factor	NUMBER		12	1
PARAM	137c6e04-d89d-469f-9fa9-b926e1d1104a	Actual Exhaust Air Flow	HVAC_AIR_FLOW		11	1
PARAM	987ca005-e391-496b-8440-338a8ef9dff8	Economizer	YESNO		6	1
PARAM	24452f06-fde6-42b5-8cd5-8d44e579f382	Coefficient of Performance	NUMBER		12	1
PARAM	cdafdf06-7a58-4c1f-820f-264a9d5af216	Serial Number	TEXT		8	1
PARAM	3dbef606-8ca1-4c48-a678-38d84262de86	Heating Entering Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	32294a07-cce7-49df-b0f8-ca6a05ae52e3	Flue Diameter	HVAC_DUCT_SIZE		1	1
PARAM	2bee6a07-d014-4303-ba02-a73157ba6cf8	Flushing Technology	TEXT		16	1
PARAM	0b538507-88db-4d93-9a9c-6903adcc42a6	Power Factor	NUMBER		5	1
PARAM	ad17b208-8987-4c58-b5d3-2b5bac288248	Return External Static Pressure	HVAC_PRESSURE		11	1
PARAM	a9395c09-4d77-4c60-9cae-74a955d7aa21	Steam Pressure Drop	PIPING_PRESSURE		6	1
PARAM	7bbe7609-fbeb-4e09-80af-e55f5b8d76ac	Heating Efficiency	NUMBER		6	1
PARAM	a46d8a09-e6b2-4ac9-9771-fa05c0888dc1	Actual Hot Gas 2 Flow	PIPING_FLOW		6	1
PARAM	ba7fa50a-a7d8-430f-80e0-41f463aea9f4	Typical Comment	TEXT		8	1
PARAM	d0bb040b-352d-4450-8a2d-20db34ca3783	ARI Number	TEXT		8	1
PARAM	1ec5740c-f29d-483b-9d22-f8f6ed99db44	Cooling Coil Fin Density per Inch	NUMBER		6	1
PARAM	895ddb0d-6098-42d1-8167-4b1e021de954	Energy Efficiency Rating	NUMBER		12	1
PARAM	67159b0e-2541-424b-b1a1-7c46a09e9809	Electric Heat Description	TEXT		6	1
PARAM	1e5de90e-2529-4d8f-ae17-85ac5b08d458	Depth	LENGTH		1	1
PARAM	2fab1c0f-f787-4343-a149-c03098bd1098	Control Protocol	TEXT		8	1
PARAM	f513b80f-aed9-476f-882b-7bdd70ff236b	Pump Power	ELECTRICAL_POWER		10	1
PARAM	b3b5a310-96b3-451e-bc69-b57d2d49f50b	Ventilation Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	14a4a813-1981-4853-a05c-0c553b8be5a1	LEED Credit	TEXT		17	1
PARAM	4cd3ab13-eb96-4ec5-b874-1ea2f7a7ab8e	Rated Load Current	ELECTRICAL_CURRENT		10	1
PARAM	132cc913-b3ae-45e8-a6e4-f82c6c1a57bf	Condenser Relief Valve Connection Diameter	PIPE_SIZE		1	1
PARAM	39d09315-298f-4c65-a20d-367885b6adbb	Hot Gas Bypass 2 Connection Diameter	PIPE_SIZE		1	1
PARAM	67470118-e2b5-4c5a-b7c8-31a98da5423a	Design Ambient Winter Dry Bulb Temperature	HVAC_TEMPERATURE		12	1
PARAM	24594f19-d09e-4f4d-8bfb-18c058b02158	PreFilter Quantity	INTEGER		11	1
PARAM	f151021b-8c09-46d7-8d72-f4ec2f192452	Design Ambient Summer Wet Bulb Temperature	HVAC_TEMPERATURE		12	1
PARAM	fa57491c-e537-4b63-8fb6-ae4476acdbd9	Cladding	TEXT		18	1
PARAM	7e9d6a1c-f3b6-4692-8774-5b877eecb068	Sensible Cooling Capacity	HVAC_COOLING_LOAD		14	1
PARAM	bfbb6e1c-3714-4f69-beb7-29c5a113337d	Return Fan Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	0168881d-60ad-4f20-b0a5-ac47b70aede7	Economizer Enthaply Limit	NUMBER		6	1
PARAM	898ef91d-3a9f-4ffe-87dc-43791d623313	Chilled Water Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	9afa161e-de87-460a-8066-a10e1587e7e9	Design Total Power	ELECTRICAL_POWER		10	1
PARAM	3e09961e-72c6-49f4-beea-bbac4f4adc24	Supply Fan Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	a7b0ca20-b7ee-46d8-b79e-3151def4d4c2	Damper Air Flow	HVAC_AIR_FLOW		11	1
PARAM	a6368922-770d-4056-b47d-aea85ea3b8cf	Electric Heat Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	04631523-ece5-442c-9c23-5d14dc6b4472	Actual Pump Water Flow	PIPING_FLOW		16	1
PARAM	3d8a4923-98a6-4d64-86fe-af81762285d4	Pump HP	ELECTRICAL_POWER		10	1
PARAM	d0fc5a24-9ae6-49f8-8ecb-6ff8169475f8	STC Rating	NUMBER		19	1
PARAM	11e64c2c-8d59-4161-a22f-f8402804965e	Nominal Cooling Capacity	HVAC_COOLING_LOAD		14	1
PARAM	69bdf42d-6913-4831-8f89-2d11928e77e3	Operating Weight	FORCE		8	1
PARAM	cb4bfe2d-0aba-4475-9629-20379916d128	Return Fan Type	TEXT		6	1
PARAM	c11b572e-4890-45c6-a255-c7b48e7f9b48	Exhaust Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	92ed7a31-adae-4e8d-bbb6-f23c0cb09b6a	Electric Heat	YESNO		20	1
PARAM	47dc5633-5872-46d7-8bdb-45417098a233	Supply Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	c4618c33-d47d-4c7a-a2de-adae18ff04d0	Exhaust Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	2fe0a033-ae1e-4e62-9ea9-f08bd99bfe26	Interior Finish	TEXT		18	1
PARAM	fb071134-1c1a-46fe-b2a6-3b42a1eae4da	Heating Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	e4f14a34-9c56-4f6c-b17a-18c67711daf7	Actual Chilled Water Flow	PIPING_FLOW		6	1
PARAM	d20d9934-4fd5-47fb-9b73-184e06f8e427	Suction Relief Valve Connection Diameter	PIPE_SIZE		1	1
PARAM	45279535-09da-4a72-9428-d844ac202e7f	Condenser Water Connection Diameter	PIPE_SIZE		1	1
PARAM	afcba335-0887-43c6-a1c0-4cde23c3c45b	Bowl Shape	TEXT		16	1
PARAM	53770139-9d6b-4ad4-bb48-a24f483ee8be	Return Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	8d4ce839-8933-4cec-bb2f-20986458dbe0	Clearance Offset Left	LENGTH		22	1
PARAM	da3a8e3a-61b4-49ce-9bd9-9806d5219de7	Filter 2 Height	LENGTH		1	1
PARAM	b7177d3b-99ec-44fe-a702-27efbbeadbef	Filter Length	LENGTH		1	1
PARAM	62a48f3b-b0d8-49dd-a2b4-cf9d155aa543	Cooling Coil Row Count	NUMBER		6	1
PARAM	bc48153c-0e6a-49db-949c-02bc58e87eb4	Actual Total Power	ELECTRICAL_POWER		10	1
PARAM	0fb0493c-02e3-4b54-9ce4-512e10acabcb	Minimum Ambient Temperature	HVAC_TEMPERATURE		6	1
PARAM	dd5ade3c-9f68-4848-ad73-fa3226dc311f	Actual Hot Gas Flow	PIPING_FLOW		6	1
PARAM	66f7253d-92e2-47eb-925e-06d3651d5fa5	Cooling Tower Fan HP	ELECTRICAL_POWER		10	1
PARAM	01e0b53d-d0b3-43e6-bc7c-4cdbf8eca75f	Clearance Offset Right	LENGTH		22	1
PARAM	f3c06f3e-174b-4508-89c2-a5896f3a5352	Heating Water Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	a3a1de3e-ff98-464d-8d0d-6ec936f6b39b	Filter Height	LENGTH		1	1
PARAM	f0cff73e-a02b-44ab-a951-3f1431584e18	Heating Nominal Input Power	ELECTRICAL_POWER		10	1
PARAM	a7d41a3f-8280-456e-a6bf-2c88f67df231	Total Cooling Capacity	HVAC_COOLING_LOAD		14	1
PARAM	63372841-100d-47cb-868c-0558228b49a3	Equipment Type	TEXT		8	1
PARAM	16943441-0138-4726-971d-ab7bf34858e5	Exhaust Fan Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	5dabce42-a666-4644-b6b8-ce339a600de5	Design Heating Water Flow	PIPING_FLOW		6	1
PARAM	a33af543-3cb7-4027-89d3-4fffcfeca6ee	Design Pressure	TEXT		19	1
PARAM	b8b61d44-e6d1-459d-a25c-cc358fa745fb	Heating Coil Face Area	AREA		6	1
PARAM	d75a5244-58b1-4b0b-b833-994d890842e5	Solar Heat Gain Coefficient	NUMBER		12	1
PARAM	110fb944-3a5d-43ec-815f-13f867c1a32b	Return Fan Power	ELECTRICAL_POWER		10	1
PARAM	a4c0ff47-e3cb-46c0-bee6-6bf1529292d0	Cooling Tower Fan Power	ELECTRICAL_POWER		10	1
PARAM	9ef3af4a-777f-4865-b52f-cde3428e6e2b	Actual Condensate Drain Flow	PIPING_FLOW		16	1
PARAM	db212a4b-10f6-4cbe-a61b-0ad178a43535	Ambient Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	abcc4c4b-b817-4daa-b720-794ba4544c78	Area Served	TEXT		8	1
PARAM	507b374e-b423-463c-8cc6-9bc5b1568212	Pump Speed	NUMBER		6	1
PARAM	f4a7854e-af78-4da1-ac1c-7e46a46e1fd7	Actual Heater Gas Flow	PIPING_FLOW		6	1
PARAM	5a1f4e4f-8f10-4e75-bdcc-cde05d0a2b85	Actual Return Air Flow	HVAC_AIR_FLOW		11	1
PARAM	f516d24f-701a-4655-8e1f-1ed5266dff66	Hot Gas Bypass Connection Diameter	PIPE_SIZE		1	1
PARAM	a24ebc50-8568-42d0-a3c5-b3b0272e2c74	Supply Total Static Pressure	HVAC_PRESSURE		11	1
PARAM	6a596a51-8abe-4038-b0c8-a561522bf90c	Ambient Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	11be8753-3808-4799-bb18-bb0ce40491d3	Evaporator Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	42e61154-a5a7-42f0-b597-17dc3c5e3c2e	Point of Shipment	TEXT		8	1
PARAM	17d53254-a00a-429c-b291-5d6422428843	Makeup Water Flow	PIPING_FLOW		16	1
PARAM	56d0c854-1a60-489d-9755-6a4d7e71f882	Heat Pump Coil Row Count	NUMBER		6	1
PARAM	2caf3855-d401-4ac2-b552-7f5270487283	Demand Control Ventilation	YESNO		11	1
PARAM	c801a656-e896-4b07-9d7b-17e8eb3a911d	Design Condenser Flow	PIPING_FLOW		6	1
PARAM	de8f3857-ed90-4510-9756-9a43a9bbc01a	Electric Heat Capacity	HVAC_HEATING_LOAD		14	1
PARAM	e91a2159-dc0e-472b-928c-6b8a6d47b626	Electric Heat Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	d052815a-546c-467d-823d-014e66dc3ce4	Clearance Width	LENGTH		22	1
PARAM	a1c4f25a-1260-41a5-bac8-97556a57b236	Apparent Load	ELECTRICAL_APPARENT_POWER		10	1
PARAM	c43e0f5b-1121-44a9-8f07-42cc88038dd8	ADA Compliant	YESNO		8	1
PARAM	3e8bcc5c-b0c2-4e09-9e32-8069c85af83a	Style	TEXT		8	1
PARAM	ab0e8a5d-e0f1-4eb0-82ae-298a98c158c2	Throw Distance Medium Velocity	LENGTH		11	1
PARAM	4a1b0e5e-e593-4599-9512-315a54cf43e6	Economizer Dry Bulb Limit	HVAC_TEMPERATURE		6	1
PARAM	a09ccf5e-8773-4e9b-8064-3078b2131430	Return Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	8f224f61-3399-4837-bf64-200445f5579b	Cooling Entering Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	56780b62-88ff-4b79-8abe-46a3dfb513f8	Ventilation Air Flow Range	TEXT		11	1
PARAM	abac2d62-ad16-4cef-ba0b-e611bf94da30	Heat Pump Coil Fin Density per Inch	NUMBER		6	1
PARAM	87319162-182d-4198-856f-da8ee80d8cc1	Heat Pump Coil Face Velocity	HVAC_VELOCITY		6	1
PARAM	f41c6867-1c6e-4e4c-9a81-b67e72793de6	Exhaust Fan Power	ELECTRICAL_POWER		10	1
PARAM	8152a668-0af3-4760-9348-ea4c3f359635	Refrigerant Used	TEXT		8	1
PARAM	b0671c69-552f-4586-82be-a31092dc32c2	Glycol Type	TEXT		6	1
PARAM	e7826969-5392-43f1-9179-8810377b3d40	Cooling Coil Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	ccd8666c-bfbb-46cb-807c-b42413e62d5a	Ventilation Total Static Pressure	HVAC_PRESSURE		11	1
PARAM	2fe7616f-d9ae-4e25-91f9-76db07a12b83	Return Fan HP	ELECTRICAL_POWER		10	1
PARAM	ee99c872-31b3-4d63-ab6d-8b6bbfb88d6c	Supply Fan Blade Speed	NUMBER		6	1
PARAM	478d7173-f09e-4899-aba7-6c8dbf672405	Supply Fan HP	ELECTRICAL_POWER		10	1
PARAM	5102b873-5fab-45b7-a2d0-f83ddee8d345	Product Name	TEXT		8	1
PARAM	2362d373-63d6-44b1-a56e-90d0fc0d80e5	Clearance Height	LENGTH		22	1
PARAM	36aa7b74-b8ac-4f6a-8a56-6115f35100cc	Unit Size	TEXT		1	1
PARAM	b1814775-9619-4b72-80e9-882e512cf476	Cooling Stages	INTEGER		14	1
PARAM	70dcae75-94be-4980-b62c-dc81bb14ff93	Evaporator Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	4cb51377-dc4d-4d9c-ba53-3856aff6ef64	Maximum Overcurrent Protection	ELECTRICAL_CURRENT		10	1
PARAM	a97c5f78-13b3-4cc9-8ca8-cb69273f5bd8	Glazing	TEXT		18	1
PARAM	4ba76a78-2f46-48dd-8af4-6bb8e5af7084	Condenser Leaving Temperature for Cooling	PIPING_TEMPERATURE		6	1
PARAM	521d5d79-9948-46b9-86c4-344c86b188b5	Design Return Air Flow	HVAC_AIR_FLOW		11	1
PARAM	435d6179-dbf0-426a-a380-8eb617e01de4	Chilled Water Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	cac0907c-6c48-451c-b354-56b4641c1e96	Actual Heating Water Flow	PIPING_FLOW		6	1
PARAM	353f987c-5499-45c3-8ea4-04f509f5c5b9	Frequency	ELECTRICAL_FREQUENCY		5	1
PARAM	8412337d-5b32-471f-a5f3-e46f43deb555	Air Terminal Air Flow	HVAC_AIR_FLOW		11	1
PARAM	ffc6ae7f-93fe-4e80-badb-61bbc0bbfc85	Flush Rate	TEXT		16	1
PARAM	0abef57f-156d-4c53-bb19-ffa01df1864b	Filter Size	TEXT		11	1
PARAM	182a0880-9337-49f7-9ef9-3673505c4c47	Glycol Percentage	NUMBER		6	1
PARAM	ddeb4880-8d29-4d55-b376-4c4aff051b14	Supply Fan Type	TEXT		6	1
PARAM	7b5d1182-c92f-4b2e-950a-0cf9c626c96e	Sound Rating	NUMBER		6	1
PARAM	bbbe2983-5687-4f7a-b851-1857c68bfcb3	Exhaust Fan Type	TEXT		6	1
PARAM	ee35ad84-b029-481a-b600-c9e17da63d7d	Material	TEXT		18	1
PARAM	06b36486-aafc-4cde-ac5c-d54281e4bae8	Minimum Air Flow	HVAC_AIR_FLOW		11	1
PARAM	7c600087-15cb-4abb-bed5-9841adba3459	Supply Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	929db387-33ff-45fc-af15-aa10763afb3b	Supply Air Connection Height	HVAC_DUCT_SIZE		1	1
PARAM	4910d787-840b-4e63-90de-0235847d1509	Notes	TEXT		8	1
PARAM	a272e187-0271-4572-b3f4-b2783042b384	Filter 2 Quantity	NUMBER		6	1
PARAM	2cfaf887-8ec9-4aa2-85af-62413c884f95	Actual Supply Air Flow	HVAC_AIR_FLOW		11	1
PARAM	3d7a268a-5abb-4f16-9623-72ffa7d32a51	Condensate Drain Connection Diameter	PIPE_SIZE		1	1
PARAM	6af1528a-2809-43aa-b9a1-78e24b557b24	Electric Heat Phase	NOOFPOLES		5	1
PARAM	612f068b-0e89-4dda-a656-0d961d27595d	Designation	TEXT		8	1
PARAM	15b2198b-2177-491f-83ef-4e64d8d36156	Design Ventilation Air Flow	HVAC_AIR_FLOW		11	1
PARAM	106f2a8b-3006-4864-aaf0-d07ea744b6f1	Width	LENGTH		1	1
PARAM	f3831d8c-b76a-4c2c-87fe-f659f1bd8328	Heating Stages	INTEGER		14	1
PARAM	59b1ab8c-3f72-4a7b-8715-3a0124d7bf9d	Actual Refrigerant Flow	PIPING_FLOW		6	1
PARAM	70a6d08c-f384-428e-b950-1a741c86b400	Evaporator Pressure Drop	PIPING_PRESSURE		6	1
PARAM	e6d72293-7fbe-4792-adc5-561e74c62910	Average Annual Operating Cost	CURRENCY		12	1
PARAM	2d482694-1287-40bd-917e-ef53c664aecb	Heating Coil Row Count	NUMBER		6	1
PARAM	19215695-f34b-4f04-8e6a-676afaf8d7f9	Design Pump Water Flow	PIPING_FLOW		16	1
PARAM	0dc29f95-b31e-45b7-b63b-80eea3303c48	Percentage of Recycled Content	NUMBER		17	1
PARAM	59d56497-cbbf-45a7-9a2c-30039a7979a1	Design Chilled Water Flow	PIPING_FLOW		6	1
PARAM	6ab9a598-d840-4d13-baa1-e3c04bd5d0ac	Supply Fan Drive	TEXT		6	1
PARAM	cc30149a-f7b4-46cc-a02d-eb9165ca485e	Cooling Leaving Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	d49c4c9a-b0a5-4a13-a2cc-b1a4580b55c6	Exhaust Total Static Pressure	HVAC_PRESSURE		11	1
PARAM	76c3739a-a466-43a6-b343-b04a5c8f773e	U Value	NUMBER		12	1
PARAM	ca1cea9a-ef12-40d6-b2c6-f800376726e0	Compressor Type	TEXT		6	1
PARAM	7cb8149b-ab87-4a5e-9338-289c4e4a6e62	Air Terminal Velocity Pressure	HVAC_PRESSURE		11	1
PARAM	e862759b-7d8a-4c70-9863-791062221fcd	Heating Input	HVAC_HEATING_LOAD		14	1
PARAM	bf6e0a9d-ed6a-4e65-a0d0-6c25cff01b00	High and Low Pressure Gas Connection Diameter	PIPE_SIZE		1	1
PARAM	37d0209d-d4ad-4422-8959-2967b0323d20	Total Heating Capacity	HVAC_HEATING_LOAD		14	1
PARAM	1eaae59d-f074-4611-b835-998bdf91c32d	Condenser Pressure Drop	PIPING_PRESSURE		6	1
PARAM	9725f69e-600c-44d9-99c3-6938c1a0c3cc	Damper Pressure Drop	HVAC_PRESSURE		11	1
PARAM	75fd1a9f-3d4b-4eee-bc23-04fe2ed8c174	Design Exhaust Air Flow	HVAC_AIR_FLOW		11	1
PARAM	8ddd76a0-f610-4ff0-8550-4b95d0c3e311	Refrigerant Liquid Connection Diameter	PIPE_SIZE		1	1
PARAM	8ca881a0-1ea3-4d67-83e2-832afcbb09bb	Electric Heat Control Steps	TEXT		6	1
PARAM	04fb0ca1-a212-451c-9d60-85fc00c5b5a9	Clearance Offset Top	LENGTH		22	1
PARAM	108cb6a1-7d8c-4c3d-9784-2f292e189386	Pump Head	PIPING_PRESSURE		6	1
PARAM	d82a02a2-6505-42cf-af1f-da72633d2700	Electric Heat Disconnect	TEXT		5	1
PARAM	894818a4-429f-4f5b-a208-dd489db008fe	Exhaust Fan HP	ELECTRICAL_POWER		10	1
PARAM	4b2e80a5-e0de-463d-ac06-da0c48378d45	PreFilter Size	TEXT		11	1
PARAM	5f4621a6-a54f-4583-9639-ba858ccbc19e	PreFilter Face Area	AREA		11	1
PARAM	334498a6-43e1-4ee8-8602-5dda9dde979d	Cooling Nominal Input Power	ELECTRICAL_POWER		10	1
PARAM	07ea2fa7-2d52-4f94-898e-3b1eb3b02473	Filter 2 Width	LENGTH		1	1
PARAM	d804d2a7-58d1-4da4-9775-e84eeb510621	Condenser Entering Temperature for Cooling	PIPING_TEMPERATURE		6	1
PARAM	2c5eeaa7-7031-42c4-896b-ea58bba2572d	Return Fan Drive	TEXT		6	1
PARAM	b88593a9-0cea-483c-8a7a-afb58bb3f979	Full Load Efficiency	NUMBER		12	1
PARAM	326628ac-3eda-49fe-a9d1-5a225554a0dd	Cooling Coil Face Area	AREA		6	1
PARAM	f596bfac-a2be-460e-96ba-09d9c1aaa72f	Exhaust Fan Motor Speed	NUMBER		6	1
PARAM	4ddd66ad-1b99-4ade-b6bf-9a73dc34010a	PreFilter Efficiency	TEXT		11	1
PARAM	2f7220ae-2cd8-4b61-a32a-451942a1c70c	Ventilation Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	98b23aae-da02-4041-9030-6ca49b6e8c2d	Low Emitting Finish	YESNO		17	1
PARAM	407a74ae-eecd-45e1-bb21-77b6bc493367	Instantaneous Current Flow	ELECTRICAL_CURRENT		10	1
PARAM	4bb069af-e98d-4159-aaeb-dc3a434c0bc5	Installation Type	TEXT		20	1
PARAM	acb411b0-dd6b-4fe6-bc02-8482e2a57f1e	Heating Water Connection Diameter	PIPE_SIZE		1	1
PARAM	93b857b0-f65a-4cba-9db9-98a23c2710dc	Heating Coil Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	40f9d3b0-a274-42a5-b990-80ae2aa13671	PreFilter Description	TEXT		11	1
PARAM	1d64eeb1-97b5-423c-8cbe-497d6d3cb989	Filter Face Area	AREA		11	1
PARAM	3e9656b2-3626-40ec-97c9-68b519a405ca	Air Terminal Static Pressure	HVAC_PRESSURE		11	1
PARAM	28424bb3-165d-400d-857f-daa57a727186	Return Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	0bba3eb5-f9eb-4fce-8460-2e8b6f5075d3	Number of Cells	INTEGER		6	1
PARAM	64cc6ab5-e9e5-44f5-a328-49a0319df1dc	Filter Quantity	NUMBER		11	1
PARAM	5ff8b5b6-a719-4ba8-9574-dd5388eb82de	Heat Pump Coil Face Area	AREA		6	1
PARAM	3bb7a9b7-ebbf-4bfb-990d-5b7a1ed8db57	Throw Distance High Velocity	LENGTH		11	1
PARAM	f41a71b8-c54b-49dd-8245-9327a406d97c	Heat of Rejection	HVAC_COOLING_LOAD		14	1
PARAM	ee1f8bb8-e503-49a8-bd5b-170d64400d82	Voltage	ELECTRICAL_POTENTIAL		5	1
PARAM	ab9bb6b8-60d4-4e34-9270-2c26aeeb600d	Cooling Entering Dry Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	8c2655ba-30b9-487c-a520-d6d056fef1f4	Return Fan Motor Speed	NUMBER		6	1
PARAM	5fb684ba-8d67-4161-be61-6bf1d2dd446c	Equipment Served	TEXT		8	1
PARAM	1f9cbaba-0477-489e-a406-ee3dcf7a59ec	R Value	NUMBER		12	1
PARAM	bff8deba-b753-4bdf-922e-b20eb6e13666	Locked Rotor Current	ELECTRICAL_CURRENT		10	1
PARAM	e8a128bb-d75a-40f3-931d-591de2fab947	Relief Valve Connection Diameter	PIPE_SIZE		1	1
PARAM	30119abb-1162-4912-a265-9adf521da240	Cooling Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	94683fbc-f392-4424-a998-aa129ce4a6da	Filter Efficiency	TEXT		11	1
PARAM	c23643bd-8129-4d1b-9217-4aa52a05633f	Salvage or Reuse	YESNO		17	1
PARAM	aa634fbd-1a84-4967-945a-4cf15c250032	Visible Light Transmission	NUMBER		12	1
PARAM	cd8265bd-6b4d-433e-9016-2f589b2ee661	Exhaust Fan Blade Speed	NUMBER		6	1
PARAM	c1b618be-baef-4a77-8c0a-b485a353e20e	Evaporator Fouling Factor	NUMBER		6	1
PARAM	513ddfbe-b6fc-408f-a3c9-3ae2d0e2071e	Filter 2 Length	LENGTH		1	1
PARAM	0bdf04bf-5d9d-4f79-b9d9-e8c361275daf	Air Terminal Total Pressure	HVAC_PRESSURE		11	1
PARAM	4de027bf-c4c2-4220-a7cc-55337537a245	Throw Distance Low Velocity	LENGTH		11	1
PARAM	a3bb9abf-c324-4a46-94de-e5d413c99640	Height	LENGTH		1	1
PARAM	de163cc0-f0ec-4db4-841c-9e8d501a560e	Design Supply Air Flow	HVAC_AIR_FLOW		11	1
PARAM	94769bc1-9237-4b9a-87eb-b6bf6a6b0e9e	Latent Cooling Capacity	HVAC_COOLING_LOAD		14	1
PARAM	3838f8c2-4f5c-4986-9000-fb036d720325	Hot Water Connection Diameter	PIPE_SIZE		1	1
PARAM	0fb442c5-a6c0-4903-87fb-b4d764c734d1	Condenser Leaving Temperature for Heating	PIPING_TEMPERATURE		6	1
PARAM	065f89c6-e350-4159-9aed-6820196ed201	Actual Valve Water Flow	PIPING_FLOW		16	1
PARAM	603013c8-8f9d-4b65-b8a9-db26d9223119	Family Load Status	TEXT		22	1
PARAM	ef74a7c8-997e-4bb8-80ab-edceb7fa352d	Electrical Disconnect	YESNO		5	1
PARAM	d3f7c6c9-ad59-4b3c-abb7-78f764f80362	EPA Rating	TEXT		8	1
PARAM	0e4bfcc9-7137-4f33-992a-e70cf17334af	Evaporator Relief Valve Connection Diameter	PIPE_SIZE		1	1
PARAM	7c4328ca-5fff-4f4e-b951-af0ee1c37d55	Exhaust Fan Drive	TEXT		6	1
PARAM	8ed442ca-c809-497c-93b3-c50b57115d3d	Refrigerant Charge	FORCE		6	1
PARAM	0e738bca-c404-402b-b3d4-7c7d4944efe6	Color	TEXT		18	1
PARAM	8b8ec2cb-f268-49d1-9fda-534b91e54583	Heating Leaving Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	cec2e9cb-9151-4b72-a3a6-2ebda7e2b2d4	Number of Poles	NOOFPOLES		5	1
PARAM	11b6a9cc-c9a2-4aba-86cd-d0601e07c827	Ventilation External Static Pressure	HVAC_PRESSURE		11	1
PARAM	bcc7dccc-a5e6-4a64-bba1-309bdbc94d46	Exhaust External Static Pressure	HVAC_PRESSURE		11	1
PARAM	b73604ce-3cea-4230-b348-1986a7918fae	Supply Fan Motor Speed	NUMBER		6	1
PARAM	ee98d0d1-ed87-46ff-9dd3-e93dd3ff6789	Nominal Part Load Value	NUMBER		12	1
PARAM	9cf1e9d1-ba10-4d28-86ee-59e0a25a6ab2	Design Ambient Summer Dry Bulb Temperature	HVAC_TEMPERATURE		12	1
PARAM	163a2cd4-c83f-4559-8130-838e1f024258	Actual Evaporator Flow	PIPING_FLOW		6	1
PARAM	e3bc86d4-a43e-4dde-a4cb-476dfa34a1cf	Shipping Weight	FORCE		8	1
PARAM	484e4ed5-0236-492c-8560-0d8fb9288c04	Actual Steam Flow	PIPING_FLOW		16	1
PARAM	9131a4d6-b41c-4164-b228-b05186f54fab	Condenser Entering Temperature for Heating	PIPING_TEMPERATURE		6	1
PARAM	dc41e7d7-c860-4fed-ab0a-d9aef1c59ffa	Ventilation Air Connection Diameter	HVAC_DUCT_SIZE		1	1
PARAM	5df563d8-778d-44d2-b0f3-058ccfe732fc	Filter Description	TEXT		11	1
PARAM	7aa550d9-9fae-44ed-9dea-fc71b89a3747	Cabinet Finish	MATERIAL		18	1
PARAM	f566bad9-494c-468d-976b-8e84de5e8de7	Clearance Offset Back	LENGTH		22	1
PARAM	385f6cda-3461-4827-bd85-8c4cc494366d	Seasonal Energy Efficiency Rating	NUMBER		12	1
PARAM	8ff8cdda-f8c3-4dc4-a3f8-70f82280de22	Low Emitting Material	YESNO		17	1
PARAM	261ed6da-7043-4241-ba2c-fbd1ca0053d7	Heat of Absorption	HVAC_HEATING_LOAD		14	1
PARAM	0e539bdb-5a35-4573-98cc-324c793721bd	Heating Coil Face Velocity	HVAC_VELOCITY		6	1
PARAM	2d4afbdb-2d08-4d25-beaa-1c756e9d87af	Length of Interconnecting Refrigerant Pipe	LENGTH		6	1
PARAM	227341dc-a5ac-4ad0-9d7b-6cba6b8a248a	Clearance Depth	LENGTH		22	1
PARAM	36d481dc-7b34-4ae0-8072-01e1cb5ce968	Clearance Type	FAMILYTYPE	-2001350	18	1
PARAM	adef5bdd-c4e9-45d9-8c8c-6f0d80e8b69e	Basin Shape	TEXT		16	1
PARAM	c319a9de-c921-4c80-ae38-7b0f3e496aa1	Pressure Rating	HVAC_PRESSURE		6	1
PARAM	2c3fd1de-c872-405f-8170-8339fa8146f8	Heating Coil Fin Density per Inch	NUMBER		6	1
PARAM	0e4028df-7a13-4649-811c-901a5c88e63d	System Served	TEXT		8	1
PARAM	ff0990e0-f4fd-4f87-8919-7383edb4b24a	Return Fan Blade Speed	NUMBER		6	1
PARAM	f695fde0-3f94-4530-abf9-7fd0e5e88457	Length	LENGTH		1	1
PARAM	e1b291e1-80ba-45c9-9da8-dc83f36a0c17	Evaporator Water Connection Diameter	PIPE_SIZE		1	1
PARAM	147865e2-5329-438a-b37f-3affebc5937f	Pump Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	9e15efe2-aeac-40fa-9d06-65b58139fc76	Chilled Water Connection Diameter	PIPE_SIZE		1	1
PARAM	78ce7ce3-aba8-4570-a7d7-038e46cd3b71	Actual Ventilation Air Flow	HVAC_AIR_FLOW		11	1
PARAM	894284e4-ba70-4b89-8725-467fd975c041	Filter Width	LENGTH		1	1
PARAM	f581cae4-9d13-456b-a180-fca24d87b9c6	Tank Type	TEXT		16	1
PARAM	2aef75e5-a454-4e57-9c20-03d15aed2d0a	Cooling Coil Face Velocity	HVAC_VELOCITY		6	1
PARAM	a09335e6-e752-425c-ba68-3e8235f530c2	Integrated Part Load Value	NUMBER		12	1
PARAM	df2279e7-23e4-4876-a7f2-a6aa5f2c2b19	Valve Pressure Drop	PIPING_PRESSURE		6	1
PARAM	645ae6e8-f7ee-4e69-bab7-44581d144da8	Air Leakage	NUMBER		12	1
PARAM	4d2d47ea-739a-4c50-809d-67499795a08a	Steam Connection Diameter	PIPE_SIZE		1	1
PARAM	5af969ea-7474-4138-9bf6-ef39e1fe04e1	Cooling Tower Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	f6b3a3ea-3d2d-4553-bd02-3ce7ddd7ad81	Exhaust Air Connection Width	HVAC_DUCT_SIZE		1	1
PARAM	a66ce4ea-9966-4361-85e3-61c5f8d34071	Boiler Water Pressure Drop	PIPING_PRESSURE		6	1
PARAM	328971eb-c691-4921-bea9-abd0308db9aa	Condenser Fouling Factor	NUMBER		6	1
PARAM	c37db9ee-7641-477c-a4d4-658a4068ede4	Chassis Finish	MATERIAL		18	1
PARAM	f850f9ee-b3e1-4373-aed6-b37eda1751ef	Water Treatment Pressure Drop	PIPING_PRESSURE		6	1
PARAM	51d103ef-fd9b-439a-8f73-ed6439a02a36	Heating Entering Wet Bulb Temperature	HVAC_TEMPERATURE		11	1
PARAM	c116acef-6cc2-4737-9fdb-8aa0af3cfc50	Actual Condenser Flow	PIPING_FLOW		6	1
PARAM	9767caef-2a2a-4744-b7fd-bafc09b113f0	Design Valve Water Flow	PIPING_FLOW		16	1
PARAM	471333f0-d333-44ee-830f-fb34165b342a	Heating Water Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	7dbbaff0-b55a-4f33-8fd4-9dc33f59a280	Condenser Leaving Temperature	PIPING_TEMPERATURE		6	1
PARAM	f598e4f0-f835-4aca-9ecd-ce1160cb384e	Condenser Entering Temperature	PIPING_TEMPERATURE		6	1
PARAM	b9a6b5f2-1be8-465f-9046-648da0d48c01	Economizer Type	TEXT		6	1
PARAM	bddc75f4-8e27-4afc-add0-de7358bbf6d3	Product Documentation Link	URL		8	1
PARAM	f01d6af5-a0ea-48d5-9f65-08a640226fbd	Maximum Overcurrent Device Type	TEXT		10	1
PARAM	1eedaaf7-5a62-4469-a31e-01d219f1df93	Clearance Offset Bottom	LENGTH		22	1
PARAM	6e8526f8-eb62-4103-90a9-41772855048f	Electric Heat Number of Poles	NOOFPOLES		5	1
PARAM	47439af8-c7fe-45ef-9341-eaab85594311	Return Total Static Pressure	HVAC_PRESSURE		11	1
PARAM	97e02bf9-0e22-41da-854f-cff85dd8b099	Full Load Current	ELECTRICAL_CURRENT		10	1
PARAM	857732fb-7721-4d42-9d8c-6ab16ccae883	Supply Fan Power	ELECTRICAL_POWER		10	1
PARAM	697795fb-88ee-4cc9-93e4-e363ae8be74b	Phase	NOOFPOLES		5	1
PARAM	20819cfb-7c5f-411d-bdcc-b1d94392e651	Heating Type	TEXT		6	1
PARAM	e40bd7fb-0f08-4c40-935b-d2047ad78b31	Sump Heater Power	ELECTRICAL_POWER		10	1
PARAM	844826fc-e1b9-4f9f-8563-09086f90f547	Location	TEXT		8	1
PARAM	f6eb65fc-3548-4622-8cbf-423c32d7b2f4	Supply External Static Pressure	HVAC_PRESSURE		11	1
PARAM	517b94fc-ff9a-46a4-aec1-65529b74103a	Electric Heat Minimum Circuit Current	ELECTRICAL_CURRENT		10	1
PARAM	2a91b0fd-1d30-4460-a431-a7a28aa69007	Energy Star Zone	TEXT		17	1
PARAM	bf05dffd-1666-4b81-8d8d-074ff06cea3a	Egress	YESNO		1	1
PARAM	6aa52afe-b294-4f4f-ade0-fe45695e3f9a	Design Evaporator Flow	PIPING_FLOW		6	1
