,Model##other##,Voltage##electrical_potential##volts,Cooling Coil Row Count##other##integer,Design Supply Air Flow##hvac_air_flow##cubic_feet_per_minute,Total Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Sensible Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Chilled Water Entering Temperature##piping_temperature##fahrenheit,Chilled Water Leaving Temperature##piping_temperature##fahrenheit,Design Chilled Water Flow##piping_flow##gallons_us_per_minute,Cooling Coil Water Pressure Drop##piping_pressure##feet_of_water,Cooling Entering Dry Bulb Temperature##hvac_temperature##fahrenheit,Cooling Entering Wet Bulb Temperature##hvac_temperature##fahrenheit,Cooling Leaving Dry Bulb Temperature##hvac_temperature##fahrenheit,Cooling Leaving Wet Bulb Temperature##hvac_temperature##fahrenheit,Heating Coil Row Count##other##integer,Total Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,Heating Water Entering Temperature##piping_temperature##fahrenheit,Heating Water Leaving Temperature##piping_temperature##fahrenheit,Design Heating Water Flow##piping_flow##gallons_us_per_minute,Heating Coil Water Pressure Drop##piping_pressure##feet_of_water,Heating Entering Dry Bulb Temperature##hvac_temperature##fahrenheit,Heating Leaving Dry Bulb Temperature##hvac_temperature##fahrenheit,Supply Fan Motor Speed##other##integer,Supply External Static Pressure##hvac_pressure##inches_of_water,Phase##other##,Nominal HP##other##,Minimum Circuit Current##electrical_current##amperes,Apparent Load##electrical_apparent_power##volt_amperes,Frequency##electrical_frequency##hertz,Depth##length##inches,Cabinet Width##length##inches,Chassis Width##length##inches,Supply Air Width##length##inches,Cabinet Height##length##inches,Fan Quantity##other##,Filter Quantity##other##,Filter Efficiency##other##,Filter Description##other##,Filter Length##length##inches,Filter Width##length##inches,Filter Height##length##inches,ARI Number##other##,Family Load Status##other##
Size 01 - 115V/60Hz/1Ph - 2 Row Coil,42VG01DYY,115,2,145,2947,2402,45,50.9,1,0.9,80,67,64.9,60.8,2,9080,180,161.8,1,0.7,70,127.3,1,0,1,0.05,15,192,60,7.125,15.75,13.875,12.75,23.75,1,1,N/R,"Throwaway, 1 - 10X14.5""",1,14.5,10,154781,Valid - Type loaded via type catalog
Size 03 - 115V/60Hz/1Ph - 2 Row Coil,42VG03DYY,115,2,285,6041,4799,45,55,1.2,2.3,80,67,64.6,60.5,2,17640,180,150.6,1.2,1.7,70,126.6,1,0,1,0.1,15,384,60,7.125,29.75,27.875,25.875,23.75,2,1,N/R,"Throwaway, 1 - 10X28""",1,28,10,154847,Valid - Type loaded via type catalog
