,Model##Other##,Description##Other##,Nominal Capacity##other##,Sensible Cooling Capacity##HVAC_COOLING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,Height##length##inches,Electrical_Wattage##ELECTRICAL_WATTAGE##WATTS,EER##other##,IEER##other##,Standards Conformance##other##,Dead Weight##other##,Constraints##other##
6.0 Ton,50GCQ07,Carrier Single Package Heat Pump Rooftop Unit -  Electric Heat 50GCQ as Specified,6.0 Ton,72000,1048mm,5700,12.6,17.6,ASHRAE 90.1  ;  AHRI 340/360  ;  DOE 2023,805,1
7.5 Ton,50GCQ08,Carrier Single Package Heat Pump Rooftop Unit -  Electric Heat 50GCQ as Specified,7.5 Ton,90000,1253mm,7400,12.2,17,ASHRAE 90.1  ;  AHRI 340/360  ;  DOE 2023,812,2
