,Model##Other##,Description##Other##,Nominal Capacity##other##,Sensible Cooling Capacity##HVAC_COOLING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,Electrical_Wattage##ELECTRICAL_WATTAGE##WATTS,EER##other##,IEER##other##,Standards Conformance##other##,Dead Weight##other##
10 Ton,50GCQ12,Carrier Single Package Heat Pump Rooftop Unit -  Electric Heat 50GCQ as Specified,10 Ton,116000,9800,11.8,16.8,ASHRAE 90.1  ;  AHRI 340/360  ;  DOE 2023,1250
