,Model##Other##,Nominal Capacity##other##,Sensible Cooling Capacity##HVAC_COOLING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,Electrical_Wattage##ELECTRICAL_WATTAGE##WATTS,EER##other##,IEER##other##,Dead Weight##other##,Horizontal Air Connections##other##
20 Ton - Vertical,50GEQ24,20 Ton,230000,21700,10.6,16.4,2307,0
25 Ton - Vertical,50GEQ28,25 Ton,294000,29100,10.1,15.5,2370,0
20 Ton - Horizontal,50GEQ24,25 Ton,230000,21700,10.6,16.4,2307,1
25 Ton - Horizontal,50GEQ28,20 Ton,294000,29100,10.1,15.5,2370,1
