,Model##Other##,Description##Other##,Refrigerant Used##other##,Nominal Capacity##other##,Sensible Cooling Capacity##HVAC_COOLING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,Height##length##inches,Electrical_Wattage##ELECTRICAL_WATTAGE##WATTS,SEER##other##,EER##other##,IEER##other##,Standards Conformance##other##,Efficiency Ratings##other##,Dead Weight##other##
14 Ton,48GCxx14xxx,Carrier Packaged Rooftop Unit - Weathermaker Gas Heat 48GC as Specified,Puron R-410A,12.5 Ton,146000,1456mm,12200,0,12,16.5,ASHRAE 90.1  ;  AHRI 340/360  ;  DOE 2023,81,1390
